1. Appropriate sampling frequency = 1500 Hz

4. Energy of x(t) = 1501.268405

7. Energy of X(f) = 4.5038e+06

8. Cut off frequency is 700 Hz.